VMS Simulator V1.00  Jun/12/1998

<FOLDER>

(1) Doc
	Folder to store documents. No docs in default.

(2) Files
	VMS simulator system files are stored.
	Bios.sbf	BIOS execution file
	vms.ini		Simulator initializing file
	vms.env		Simulator environment setting file
	Default.env	Application default environment file
	Buz2k.wav	2KHz sign wave audio file
	Buz4k.wav	4KHz sign wave audio file
	Pwm.wav		PWM confirmation audio file

(3) Help
	Vmshelp.hlp	Japanese version help file
	VmshelpUS.hlp	English version help file

(4) Project
	Working folder for user application.  Nothing's contained in default.
	Storing sample/test programs in this folder is recommended.

<Regarding HELP files>
It can be specified by Lang in the vms.ini file.  When it is executed as a Japanese version, Japanese help will be refered.  When English version, English help will be referred.  Both files are under the Help folder, so English version is named !"VmshelpUS.hlp".  In this way, VMS simulator can support both languages including help files.


<BIOS>

BIOS files are converted from simple HEX files to cryptography SBF files.  The BIOS files under the current Files folder are the cryptographized files that are converted from the latest.  Help specifies two types of BIOS, full size BIOS and quick start BIOS, yet currently only full size BIOS is available.
BIOS name can be specified by RegMap.exe, so please specify the file name using this tool when creating SDK.  Store BIOS SBF file to Files folder.


<Install Shield>
The installer has been made using:
	InstallShield Express C++ Builder Edition  Version 1.11
The project file for IS is vms.iwz, which has been used for creation.
Please refer to this project file when making one for your own.  DLL/OCX related files should be watched carefully.


<FLASH#1>
Upon request, FLASH#1 processing has been deleted.  Help file needs to be reflected this change.  Also, FLASH#1 tab page has been removed from the memory control panel.


<ReadMe.txt>
No readme files for user.
