Registers a callback function to use for the YUV termination interrupt.

Prototype declaration:

> `

>     KMSTATUS KMAPI
>     kmSetEndOfYUVCallback(
>     		IN   PKMCALLBACKFUNC    pEndOfYUVCallback,
>     		IN   PVOID              pCallbackArguments
>     );

> `

Description:

>     This function registers a callback function to use for the YUV termination interrupt issued
>     when the YUV converter finishes the conversion process.

>     	VOID EndOfYUVFunc(PVOID pCallbackArguments);

>     pCallbackArguments(input): Pointer to the parameter set at the specification

Parameters:

>     pEndOfYUVCallback(input)
>             This parameter specifies a pointer to a callback function to use when the YUV converter
>             finishes its task.

>     pCallbackArguments(input)
>             This parameter is a pointer to an argument to be passed to the function called at callback.

Return values:

> Value | Explanation
> KMSTATUS_SUCCESS | Success