##### Sound Function - Sound Module Control Function

# sdShotResetPrm

Resets a One-Shot port

### FORMAT

`

  SDE_ERR sdShotResetPrm( handle )
  SDSHOT handle

`

### PARAMETER

  `handle` | Object handle

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HANDLE_NULL | The handle is NULL |
  SDE_ERR_HOST_CMD_BUF_NO_ENOUGH | No more host commands can be accepted |

### DESCRIPTION

  Resets the level parameters for a One-Shot port.

### NOTE

  All levels are reset to 0 (center).

sdShotResetPrm

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999