##### Shinobi Library - Memory Card Function

# buStat

Checks whether processing is completed

### FORMAT

`

  Sint32 buStat( drive )
  Sint32 drive

`

### PARAMETER

  `drive` | Extension socket number

### RETURN

  BUD_STAT_READY | Processing has been completed |
  BUD_STAT_BUSY | A type_B function is being processed |

### DESCRIPTION

  Checks whether processing has been completed on a memory card inserted in a specified extension socket.

  The following values can be designated for the argument `drive` that specifies extension sockets.

  BUD_DRIVE_A1 | Extension socket 1 on board A
  BUD_DRIVE_A2 | Extension socket 2 on board A
  BUD_DRIVE_B1 | Extension socket 1 on board B
  BUD_DRIVE_B2 | Extension socket 2 on board B
  BUD_DRIVE_C1 | Extension socket 1 on board C
  BUD_DRIVE_C2 | Extension socket 2 on board C
  BUD_DRIVE_D1 | Extension socket 1 on board D
  BUD_DRIVE_D2 | Extension socket 2 on board D

### EXAMPLE

      if (buStat(BUD_DRIVE_A1) == BUD_STAT_BUSY) {
      	:
         /* Processing still in progress */
      	:
      }

buStat

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999