##### Sound Function - Sound System Function

# sdSysFlushHostCmd

Sends the host command

### FORMAT

`

  SDE_ERR sdSysFlushHostCmd( Void )

`

### PARAMETER

  None

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_SND_DRV_BUSY | The Sound Driver cannot accept the host command |

### DESCRIPTION

  Sends communication packets (Host Command) to the ARM7 Sound Driver, buffered by the Sound Library.

### NOTE

  Sends the data received by the Sound Driver. Some time is required for the ARM7 Sound Driver to process the sent data, so the response is delayed slightly (not more than several milliseconds).

sdSysFlushHostCmd

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999