##### Shinobi Library - Vibration Peripheral Structure

# PDS_VIBUNITINFO

Structure where vibration peripheral unit information is stored

### DEFINITION

      typedef struct {
       Uint8 position;
       Uint8 axis;
       Uint8 pow_enable;
       Uint8 cont_enable;
       Uint8 dir_enable;
       Uint8 wave_enable;
       Uint8 min_freq;
       Uint8 max_freq;
      } PDS_VIBUNITINFO;

### MEMBER

  `position` | Vibration peripheral unit position
  `axis` | Vibration axis
  `pow_enable` | Intensity variable
  `cont_enable` | Continuous vibration enable
  `dir_enable` | Direction specification enable
  `wave_enable` | Optional waveform setting enable
  `min_freq` | Minimum vibration frequency
  `max_freq` | Maximum vibration frequency

### DESCRIPTION

  Structure where unit information for the vibration peripheral is stored.

### REFERENCE

  `pdVibEnumerateUnit()
  `

PDS_VIBUNITINFO

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999