##### Shinobi Library - Vibration Peripheral Function

# pdVibIsReady

Gets connection status of the vibration peripheral

### FORMAT

`

  pdVibIsReady( port )
  Uint32 port

`

### PARAMETER

  `port` | Port number

### RETURN

  TRUE | Vibration peripheral is connected |
  FALSE | Vibration peripheral is not connected |

### DESCRIPTION

  Checks whether a vibration peripheral is connected.

  The following values can be set for the argument `port`.

  PDD_PORT_A1 | Expansion socket 1 on port A
  PDD_PORT_A2 | Expansion socket 2 on port A
  PDD_PORT_B1 | Expansion socket 1 on port B
  PDD_PORT_B2 | Expansion socket 2 on port B
  PDD_PORT_C1 | Expansion socket 1 on port C
  PDD_PORT_C2 | Expansion socket 2 on port C
  PDD_PORT_D1 | Expansion socket 1 on port D
  PDD_PORT_D2 | Expansion socket 2 on port D

### EXAMPLE

      if (pdVibIsReady(PDD_PORT_A2))
      	return TRUE;

### NOTE

  These functions are still in the evaluation version. In the future, specs may be changed.

pdVibIsReady

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999