##### Shinobi Library - Video Cable Check Function

# syCblCheckBroadcast

Gets broadcast system

### FORMAT

`

  SYE_CBL_BROADCAST syCblCheckBroadcast( void )

`

### PARAMETER

  None

### RETURN

  Broadcast system

### DESCRIPTION

  Gets the broadcast system.

  The return values have the following meaning:

  SYE_CBL_BROADCAST_NTSC | NTSC(Japan, US)
  SYE_CBL_BROADCAST_PAL | PAL(Europe)
  SYE_CBL_BORADCAST_PALM | PAL-M(Brazil)
  SYE_CBL_BROADCAST_PALN | PAL-N(Argentina)

### NOTE

  The broadcast system is set when Dreamcast hardware is factory-issued.

syCblCheckBroadcast

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999