##### Sound Function - Sound Module Control Function

# sdGddaSetPan

Sets the GD-DA panpot level

### FORMAT

`

  SDE_ERR sdGddaSetPan( left_pan, right_pan )
  Sint8 left_pan
  Sint8 right_pan

`

### PARAMETER

  `left_pan` | Left side GD-DA volume level
  `right_pan` | Right side GD-DA volume level

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HOST_CMD_BUF_NO_ENOUGH | No more host commands can be accepted |

### DESCRIPTION

  Sets GD-DA panpot levels. The value range that can be set for each parameter is -007FH (left) to 0000H (center) to 007FH (right).

sdGddaSetPan

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999