##### Shinobi Library - Vibrating Peripheral Control Structure

# PDS_VIBPARAM

Structure that stores vibration parameters

### DEFINITION

      typedef struct {
       Uint8 unit;
       Uint8 flag;
       Sint8 power;
       Uint8 freq;
       Uint8 inc;
       Uint8 reserved[3];
      } PDS_VIBPARAM;

### MEMBER

  `unit` | Unit number that sends the vibration parameter
  `flag` | Vibration flag
  `power` | Vibration intensity
  `freq` | Vibration frequency
  `inc` | Vibration incline cycle
  `reserved` | Reserved

### DESCRIPTION

  Structure that stores the vibration parameters of the vibration peripheral.

### REFERENCE

  `pdVibMxStart()
  pdVibStart()
  `

PDS_VIBPARAM

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999