##### Sound Library - GD-DA Structure

# SDS_GDDA_STAT

Data types defining GD-DA status

### DEFINITION

      struct SDS_GDDA_STAT
      {
              Sint8   m_HostCmdRsvNum;
              Sint8   m_HostCmdDelayTime;
              Sint8   m_LeftVol;
              Sint8   m_RightVol;
              Sint8   m_LeftPan;
              Sint8   m_RightPan;
              Error Status
              Various flags
      };
      typedef struct SDS_GDDA_STAT    SDS_GDDA_STAT;

### MEMBER

  `m_HostCmdRsvNum` | Host Command Reserve Size
  `m_HostCmdDelayTime` | Host command sending delay time (Currently undefined)
  `m_LeftVol` | Left channel volume of current GD-DA
  `m_RightVol` | Right channel volume of current GD-DA
  `m_LeftPan` | Left channel panpot of current GD-DA
  `m_RightPan` | Right channel panpot of current GD-DA
  `m_Err` | Error Status
  `m_Flg` | Various flags

### DESCRIPTION

  GD-DA status information data types

### REFERENCE

  `sdGddaGetStat()
  `

SDS_GDDA_STAT

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999