##### Shinobi Library - Vibration Peripheral Function

# pdVibMxIsReady

Gets connection status of the vibration peripheral

### FORMAT

`

  Sint32 pdVibMxIsReady( port )
  Uint32 port

`

### PARAMETER

  port Port number

### RETURN

  none

### DESCRIPTION

  Checks whether a vibration peripheral is connected.

  The following values can be set for the argument `port`.

  PDD_PORT_A1 | Expansion socket 1 on port A
  PDD_PORT_A2 | Expansion socket 2 on port A
  PDD_PORT_B1 | Expansion socket 1 on port B
  PDD_PORT_B2 | Expansion socket 2 on port B
  PDD_PORT_C1 | Expansion socket 1 on port C
  PDD_PORT_C2 | Expansion socket 2 on port C
  PDD_PORT_D1 | Expansion socket 1 on port D
  PDD_PORT_D2 | Expansion socket 2 on port D

### EXAMPLE

      if (pdVibMxIsReady(PDD_PORT_A2))
      	return TRUE;

### NOTE

  In the present version, "TRUE" is returned if a vibration peripheral is connected. These functions are still in the evaluation version. In the future, the specs may be changed.

pdVibMxIsReady

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999