##### Sound Function - Sound Module Control Function

# sdPstmGetTotalSmpFrame

Gets total PCM Stream play sample frames

### FORMAT

`

  SDE_ERR sdPstmGetTotalSmpFrame( handle, ch_num, *total_smp_frame )
  SDPSTM handle
  Sint8 ch_num
  Uint32 *total_smp_frame

`

### PARAMETER

  `handle` | Object handle
  `ch_num` | Channel number for which to get current playing address
  `total_smp_frame` | Pointer to storage for obtained total playing sample frame number

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HANDLE_NULL | The handle is NULL |
  SDE_ERR_HOST_CMD_BUF_NO_ENOUGH | No more host commands can be accepted |

### DESCRIPTION

  Gets the total sample frames playing on the PCM Stream.

sdPstmGetTotalSmpFrame

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999