##### Sound Function - Sound Module Control Function

# sdPstmSetDrctLev

Sets the direct level of a PCM Stream port

### FORMAT

`

  SDE_ERR sdPstmSetDrctLev( handle, drct_lev )
  SDPSTM handle
  Sint8 drct_lev

`

### PARAMETER

  `handle` | Object handle
  `drct_lev` | Direct level to set

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HANDLE_NULL | The handle is NULL |
  SDE_ERR_HOST_CMD_BUF_NO_ENOUGH | No more host commands can be accepted |

### DESCRIPTION

  Sets the direct (without sound effects) level of a PCM Stream port. The range of values for `drct_lev`, which specifies direct levels, is -007FH (min) to 0000H (mid) to 007FH (max).

sdPstmSetDrctLev

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999