##### Sound Function - Sound Module Control Function

# sdShotSetFxLev

Sets the FX level of a One-Shot port

### FORMAT

`

  SDE_ERR sdShotSetFxLev( handle, fx_lev )
  SDSHOT handle
  Sint8 fx_lev

`

### PARAMETER

  `handle` | Object handle
  `fx_lev` | FX level to set

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HANDLE_NULL | The handle is NULL |
  SDE_ERR_PRM_OVER_RANGE | Parameter out of range |
  SDE_ERR_HOST_CMD_BUF_NO_ENOUGH | No more host commands can be accepted |

### DESCRIPTION

  Sets the FX level of a One-Shot port. The range of `fx_lev`, which specifies the FX level to set, is -007FH (min) to 0000H (mid) to 007FH (max).

sdShotSetFxLev

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999