##### Shinobi Library - Peripheral Data Acquistion Structure

# PDS_PERIPHERALINFO

Structure where inherent peripheral information is stored

### DEFINITION

      typedef struct {
       Uint32 type;
       Uint32 reserved[3];
       Uint8 is_root;
       Uint8 area_code;
       Uint8 connector_dir[2];
       Sint8 product_name[32];
       Sint8 license[64];
       Uint16 stdby_pow;
       Uint16 max_pow;
      } PDS_PERIPHERALINFO;

### MEMBER

  `type` | Peripheral type
  `reserved[3]` | Reserved
  `is_root` | Root device flag
  `area_code` | Area code
  `connector_dir[2]` | Extended connector oriented
  `product_name[32]` | Product name
  `license[64]` | License string
  `stdby_pow` | Standby power consumption
  `max_pow` | Maximum power consumption

### DESCRIPTION

  Structure where inherent peripheral information is stored.

### REFERENCE

  `pdGetPeripheralInfo()
  `

PDS_PERIPHERALINFO

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999