##### Sound Function - Sound Module Control Function

# sdShotSetVol

Sets the volume of a One-Shot port

### FORMAT

`

  SDE_ERR sdShotSetVol( handle, vol, fade_time )
  SDSHOT handle
  Sint8 vol
  Sint16 fade_time

`

### PARAMETER

  `handle` | Object handle
  `vol` | Target volume
  `fade_time` | Time to reach target volume

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HANDLE_NULL | The handle is NULL |
  SDE_ERR_HOST_CMD_BUF_NO_ENOUGH | No more host commands can be accepted |

### DESCRIPTION

  Sets the play volume of a One-Shot port.

  The range of `vol`, which specifies volume, is -007FH (min) to 0000H (mid) to 007FH (max).

  Units of `fade_time`, which specifies the time needed to reach volume, are milliseconds, from 0000H (fastest) to 7FFFH (slowest).

sdShotSetVol

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999