Continues Pass.

Prototype declaration:

> `

>     KMSTATUS KMAPI
>     kmContinuePass(
>     		IN OUT  PKMVERTEXBUFFDESC   pVertexBuffDesc
>     );

> `

Description:

>     This functions continues Pass.
>     In a multi-pass situation, kmEndPass/kmBeginPass can also be used for pass continuation.
>     The code for a multi-pass situation can be written in the two ways shown below.

>     (Example)  In the case of three passes

>     (1)                            (2)
>         kmBeginScene();                 kmBeginScene();
>             kmBeginPass();                  kmBeginPass();
>                 ...                             ...
>               (Pass1)                         (Pass1)
>                 ...                             ...
>             kmContinuePass                  kmEndPass();
>                 ...                         kmBeginPass();
>               (Pass2)                           ...
>                 ...                           (Pass2)
>             kmContinuePass                      ...
>                 ...                         kmEndPass();
>               (Pass3)                       kmBeginPass();
>                 ...                             ...
>             kmEndPass();                      (Pass3)
>         kmEndScene();                           ...
>                                             kmEndPass();
>                                         kmEndScene();

Parameters:

>     pVertexBuffDesc(input)
>             This parameter is a pointer to KMVERTEXBUFFDESC.

Return values:

> Value | Explanation
> KMSTATUS_SUCCESS | Success