/****************************************************************
  <pvrconv Release Log>           
*****************************************************************/

12/10/97 0.7alpha3
=====================
> Added -ns option. The suffix of the texure is ignored by this option.
The texture name must not have the suffix when the texture is converted. 
> If the texture size is one ot the following numbers, pic, tga, bmp, pix are detected and automatically converted even if the texture does not have a suffix.

1, 2, 4, 8, 16, 32, 64, 128, 256, 512, 1024
 

11/07/97 0.7alpha2
=====================
> Added new section that creates pvr with alpha from two bmp files.
> Added ability to convert 512 x 512 and 1024 x 1024 tga files.
> Corrected the bug that prevented proper twiddled conversion of 512 x 512 and 1024 x 1024 images in which the upper left quadrant was converted and the remaining three quadrants became black.
> Corrected bug in which, when there was no mipmap, the globalIndex chunk was not written to the pvr file.

--


