Specifies the display line on which an interrupt is caused.

Prototype declaration:

> `

>     KMSTATUS KMAPI
>     kmSetHSyncLine(
>     		IN  KMINT32     nInterruptLine
>     );

> `

Description:

>     This function specifies the display line on which an interrupt is caused.

Parameters:

>     nInterruptLine(input)
>             This parameter specifies the line on which an interrupt is caused.  Specify a value within
>             the range of 0 to 240/480.

Return values:

> Value | Explanation
> KMSTATUS_SUCCESS | Success
> KMSTATUS_ILLEGAL_PARAMETER | Invalid parameter