##### Sound Function - Global Sound Control Function

# sdQsndSetPos

Sets Q Sound position

### FORMAT

`

  SDE_ERR sdQsndSetPos( *pos )
  Sint8 *pos

`

### PARAMETER

  `pos` | Position to set

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HOST_CMD_BUF_NO_ENOUGH | No more Host Commands can be accepted |
  SDE_ERR_PRM_OVER_RANGE | Parameter out of range |

### DESCRIPTION

  Sets Q Sound position. The argument `pos` that specifies position has a 6 byte array of 8-bit signed integers and each element corresponds to a Q Sound module.

sdQsndSetPos

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999