##### Shinobi Library - Real-time Clock Function

# syRtcSetServerMode

Sets server release operation

### FORMAT

`

  void syRtcSetServerMode( mode )
  const Sint32 mode

`

### PARAMETER

  `mode` | Server function operation

### RETURN

  None

### DESCRIPTION

  Sets the server function activity status.

  The operation that sets the server server function in `model` can specify the following statuses.

  SYD_RTC_STAT_ACTIVE | Accesses the real-time clock (default)
  SYD_RTC_STAT_PASSIVE | Doesn't access the real-time clock

syRtcSetServerMode

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999