##### Shinobi Library - Cache Function

# syCacheOCWB

Writes back all cache blocks that include the specified area

### FORMAT

`

  Void syCacheOCWB( *address, size )
  Void *address
  Uint32 size

`

### PARAMETER

  `*address` | Starting address
  `size` | Size

### RETURN

  None

### DESCRIPTION

  Writes back all cache blocks that include the specified area. ("To write back" means to write the contents of the cache back to physical memory.)

### NOTE

  If the address of P2 are(range from 0xa0000000 to 0xbfffffff) is specified, this area is replaced with the P0 area and is written back. In other words, even in the case of the non-cacheable P2 area, the change is still made in the actual memory.

syCacheOCWB

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999