##### Sound Function - Sound Module Control Function

# sdPstmGetStat

Gets PCM Stream port status

### FORMAT

`

  SDE_ERR sdPstmGetStat( handle, ch_num, *stat )
  SDPSTM handle
  Sint8 ch_num
  SDS_PSTM_STAT *stat

`

### PARAMETER

  `handle` | Object handle
  `ch_num` | Channel number
  `stat` | Pointer to storage for obtained channel status of PCM Stream port

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HANDLE_NULL | The handle is NULL |

### DESCRIPTION

  Gets port status of the PCM Stream.

sdPstmGetStat

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999