##### Sound Function - Sound Module Control Function

# sdMidiContinue

Resumes MIDI sequence play

### FORMAT

`

  SDE_ERR sdMidiContinue( handle )
  SDMIDI handle

`

### PARAMETER

  `handle` | Object port handle

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HANDLE_NULL | The handle is NULL |
  SDE_ERR_HOST_CMD_BUF_NO_ENOUGH | No more host commands can be accepted |

### DESCRIPTION

  Resumes MIDI sequence play.

### NOTE

  SdMidiPause must be called first for pause/resume operation.

### REFERENCE

  `sdMidiPause()
  `

sdMidiContinue

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999