##### Sound Function - Sound Module Control Function

# sdMidiPause

Pauses MIDI sequence play

### FORMAT

`

  SDE_ERR sdMidiPause( handle )
  SDMIDI handle

`

### PARAMETER

  `handle` | Object port handle

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HANDLE_NULL | The handle is NULL |
  SDE_ERR_HOST_CMD_BUF_NO_ENOUGH | No more host commands can be accepted |

### DESCRIPTION

  Pauses MIDI sequence play.

sdMidiPause

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999