##### Sound Function - Sound Module Control Function

# sdGddaSetVol

Sets the GD-DA volume

### FORMAT

`

  SDE_ERR sdGddaSetVol( left_vol, right_vol )
  Sint8 left_vol
  Sint8 right_vol

`

### PARAMETER

  `left_vol` | Left side GD-DA volume level
  `right_vol` | Right side GD-DA volume level

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HOST_CMD_BUF_NO_ENOUGH | No more host commands can be accepted |

### DESCRIPTION

  Sets the GD-DA volume level.

sdGddaSetVol

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999