##### Sound Function - Sound Module Control Function

# sdShotSetStat

Gets One-Shot port status

### FORMAT

`

  SDE_ERR sdShotGetStat( handle, *stat )
  SDSHOT handle
  SDS_SHOT_STAT *stat

`

### PARAMETER

  `handle` | Object handle
  `stat` | Pointer to storage of obtained One-Shot port status

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HANDLE_NULL | The handle is NULL |

### DESCRIPTION

  Gets One-Shot port status.

sdShotSetStat

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999