##### Sound Function - Sound System Function

# sdDrvGetMidiTimmingCounter

Gets special message count

### FORMAT

`

  SDE_ERR sdDrvGetMidiTimmingCounter( *count_num )
  Uint32 *count_num

`

### PARAMETER

  `count_num` | Pointer of valiables to store the Sound Driver count

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_PTR_NULL | NULL |

### DESCRIPTION

  Gets count value counted by Sound Driver based on special messages of sound data.

### NOTE

  It is possible to use special timing for Sound Creator using this function.

sdDrvGetMidiTimmingCounter

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999