##### Sound Function - Memory Block Transfer Function

# sdMemBlkGetStat

Checks the status of a Memory Block handle

### FORMAT

`

  SDE_ERR sdMemBlkGetStat( handle, *stat )
  SDMEMBLK handle
  SDE_MEMBLK_STAT *stat

`

### PARAMETER

  `handle` | Memory Block handle
  `stat` | Pointer to the resulting block status data

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |
  SDE_ERR_HANDLE_NULL | The handle was NULL |
  SDE_ERR_HANDLE_ILLEGAL_VALUE | An illegal address was specified for the handle |

### DESCRIPTION

  Checks the status of the Memory Block handle.

  The argument `stat` that stores results returns the following values.

  SDE_MEMBLK_STAT_TRANSFER_REMAIN | Memory block transfer remaining
  SDE_MEMBLK_STAT_TRANSFER_FINISHED | Memory block transfer finished
  SDE_MEMBLK_STAT_TRANSFER_PROGRESS | Memory Block Transfer API

sdMemBlkGetStat

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999