##### Sound Function - Memory Block Transfer Function

# sdMemBlkSetTransferMode

Sets the transfer mode for Memory Blocks

### FORMAT

`

  SDE_ERR sdMemBlkSetTransferMode( transfer_mode )
  SDE_MEMBLK_TRANSFER_MODE transfer_mode

`

### PARAMETER

  `transfer_mode` | Transfer Mode

### RETURN

  SDE_ERR_NO_INIT | The Sound Library has not been initialized |

### DESCRIPTION

  Sets the transfer method for Memory Blocks.

  The following values are specified for the parameter "transfer_mode".

  SDE_MEMBLK_TRANSFER_MODE_CPU | Transfer by CPU(SH-4)
  SDE_MEMBLK_TRANSFER_MODE_DMA | Transfer by DMA

sdMemBlkSetTransferMode

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999