##### Ninja Library - Camera Function

# njSetCameraDepth

Sets near clipping and far clipping limit

### FORMAT

`

  void njSetCameraDepth(*c, n, f)
  NJS_CAMERA *c
  Float n
  Float f

`

### PARAMETER

  `*c` | Pointer to camera structure
  `n` | Near clipping limit
  `f` | Far clipping limit

### RETURN

  None

### DESCRIPTION

  Specifies the near clipping and far clipping limit. In the Ninja coordinate system, Z axis values are negative in the far direction of the screen. Therefore n and f are specified as negative values.

  (-1.0 => n > f => -65535.0)

  If the specified value is larger than -1.0 or smaller than - 65535.0, it is automatically taken as -1.0 and -65535.0, respectively.

### EXAMPLE

      #define N_CLIP   -500.f
      #define F_CLIP   -50000.f
      NJS_CAMERA c;
      njInitCamera(&c);
      njSetCameraDepth(&c, N_CLIP, F_CLIP);
      njSetCamera(&c);

njSetCameraDepth

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999