##### Shinobi Library - Memory Card Function

# buGetFileInfo

Gets file information

### FORMAT

`

  Sint32 buGetFileInfo( drive, *fname, *info )
  Sint32 drive
  const char *fname
  BUS_FILEINFO *info

`

### PARAMETER

  `drive` | Extension socket number
  `*fname` | File name
  `*info` | Address of file information structure

### RETURN

  BUD_ERR_OK | File found |
  BUD_ERR_FILE_NOT_FOUND | File not found |
  BUD_ERR_UNFORMAT | Disk is not formatted |
  BUD_ERR_NO_DISK | Memory card not found |
  BUD_ERR_BUSY | A type_B function is being processed |

### DESCRIPTION

  Gets information for a file from a memory card inserted in a specified extension socket.

  The following values can be designated for the argument `drive` that specifies extension sockets.

  BUD_DRIVE_A1 | Extension socket 1 on board A
  BUD_DRIVE_A2 | Extension socket 2 on board A
  BUD_DRIVE_B1 | Extension socket 1 on board B
  BUD_DRIVE_B2 | Extension socket 2 on board B
  BUD_DRIVE_C1 | Extension socket 1 on board C
  BUD_DRIVE_C2 | Extension socket 2 on board C
  BUD_DRIVE_D1 | Extension socket 1 on board D
  BUD_DRIVE_D2 | Extension socket 2 on board D

### EXAMPLE

      BUS_FILEINFO info;
      buGetFileInfo( BUD_DRIVE_A1, "SAVEDATA_001", &info );

buGetFileInfo

COPYRIGHT © SEGA ENTERPRISES, LTD., 1998,1999