Changes CullingMode.(KMSTRIPHEAD Structure)

Prototype declaration:

> `

>     KMSTATUS KMAPI
>     kmChangeStripCullingMode(
>             IN OUT  PKMSTRIPHEAD    pStripHead,
>             IN      KMCULLINGMODE   nCullingMode
>     );

> `

Description:

>     This function changes CullingMode in a KMSTRIPHEAD structure that was constructed by
>     kmGenerateStripHead/kmGenerateStripHeadXX (00 to 17).
>     The following is a list of supported VertexType:

>             VertexType00
>                 VertexType06
>                 VertexType12
>             VertexType01
>                 VertexType07
>                 VertexType13
>             VertexType02
>                 VertexType08
>                 VertexType14
>             VertexType03
>                 VertexType09
>                 VertexType15
>             VertexType04
>                 VertexType10
>                 VertexType16
>             VertexType05
>                 VertexType11
>                 VertexType17

Parameters:

>     pStripHead(input/output)
>             This parameter is a pointer to KMSTRIPHEAD.

>     nCullingMode(input)
>             This parameter specifies the CullingMode setting.
>                 KM_NOCULLING
>                 KM_CULLSMALL
>                 KM_CULLCCW
>                 KM_CULLCW

Return values:

> Value | Explanation
> KMSTATUS_SUCCESS | Success