kmSetColorClampMax

Specifies the color clamp maximum value.

KMSTATUS KMAPI
kmSetColorClampMax(
IN KMPACKEDARGB Val
)

Description:

This function specifies the color clamp maximum value.
Color clamping is applied ahead of fogging. If you want to change the clamp color when rendering, do so within a callback function for rendering termination. If an attempt is made to change the clamp color at any other timing, a screen image may become invalid.

Parameters:

Val(input)
This parameter specifies a maximum value for color clamping. It is a packed ARGB 32-bit color. If you want to specify the RGB color with a brightness of 128, enter 0x00808080.

Return values:

Value | Explanatrion
--- | ---
KMSTATUS_SUCCESS | Success

kmSetColorClampMax